; xtouch.inf
;
; Installation file (.inf) for the eGalaxTouch device.
;
; (c) Copyright 2000 ~ 2009 Inc. 
;

[Version]
Signature="$Windows NT$"
Provider=%EGALAXTOUCH%
ClassGUID={4D36E96F-E325-11CE-BFC1-08002BE10318}
Class=Mouse
CatalogFile=xtouch.cat
DriverVer=01/08/2009, 5.1.1.6208
[SourceDisksNames]
1 = %DiskId1%,,
[DestinationDirs]
DefaultDestDir   = 12
DLLCopyFiles = 11
;
; Driver information
;

[Manufacturer]
%EGALAXTOUCH%   = eGalaxTouchMfg;

[eGalaxTouchMfg]
%USB_UNIV_TOUCH%     = usb_univ_Inst, USB\VID_0EEF&PID_0001
%USB_PROF_TOUCH%     = usb_univ_Inst, USB\VID_0EEF&PID_0002
%USB_1000_TOUCH%     = usb_univ_Inst, USB\VID_0EEF&PID_1000
%USB_2000_TOUCH%     = usb_univ_Inst, USB\VID_0EEF&PID_2000
%USB_4000_TOUCH%     = usb_univ_Inst, USB\VID_0EEF&PID_4000
%USB_6000_TOUCH%     = usb_univ_Inst, USB\VID_0EEF&PID_6000
%USB_7000_TOUCH%     = usb_univ_Inst, USB\VID_0EEF&PID_7000
%USB_8000_TOUCH%     = usb_univ_Inst, USB\VID_0EEF&PID_8000
%USB_9000_TOUCH%     = usb_univ_Inst, USB\VID_0EEF&PID_9000
;
; General installation section
;

;====================================================================
;================= USB Touchscreen Section ==========================
;====================================================================
[usb_univ_Inst]
AddReg=xtouch_AddReg
; Copy the driver over
CopyFiles=XCopyFiles_Drivers, DLLCopyFiles

[xtouch_AddReg]
;
; File sections
;


[XCopyFiles_Drivers]
xtouch.sys

[DLLCopyFiles]
;eGalaxTouchprop.dll
;
; Service Installation
;
[usb_univ_Inst.Services]
AddService = xtouch, 0x00000002 , xtouch_Service_Inst, xtouch_EventLog_Inst
; Install mouclass.sys from msmouse.inf
Include=msmouse.inf
Needs=MouClass.Services

[usb_univ_Inst.HW]
AddReg=usb_AddReg
;DelReg=usb_DelReg

[xtouch_Service_Inst]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 0                  ; SERVICE_ERROR_IGNORE
LoadOrderGroup = Pointer Port
ServiceBinary  = %12%\xtouch.sys

[xtouch_EventLog_Inst]
AddReg = xtouch_EventLog_AddReg

[xtouch_EventLog_AddReg]
HKR,,EventMessageFile,0x00020000,"%SystemRoot%\System32\IoLogMsg.dll;%SystemRoot%\System32\drivers\xtouch.sys"
HKR,,TypesSupported,0x00010001,7

[usb_AddReg]
;HKR,,"BeepMode",0x00010003,1
;HKR,,"MouseMode",0x00010003,0x00000000


;
; Source file information
;
[SourceDisksFiles]
; Files for disk eGalaxTouch Touchscreen Controller. Installation Disk #1 (Mouse)
xtouch.sys = 1,,


[Strings]

;
; Non-Localizable Strings
;

REG_SZ         = 0x00000000
REG_MULTI_SZ   = 0x00010000
REG_EXPAND_SZ  = 0x00020000
REG_BINARY     = 0x00000001
REG_DWORD      = 0x00010001
SERVICEROOT    = "System\CurrentControlSet\Services"

;
; Localizable Strings
;

USB_UNIV_TOUCH  = "USB Touchscreen Controller(Universal)"
USB_PROF_TOUCH  = "USB Touchscreen Controller(Professional)"
USB_1000_TOUCH  = "USB Touchscreen Controller(1000)"
USB_2000_TOUCH  = "USB Touchscreen Controller(2000)"
USB_4000_TOUCH  = "USB Touchscreen Controller(4000)"
USB_6000_TOUCH  = "USB Touchscreen Controller(6000)"
USB_7000_TOUCH  = "USB Touchscreen Controller(7000)"
USB_8000_TOUCH  = "USB Touchscreen Controller(8000)"
USB_9000_TOUCH  = "USB Touchscreen Controller(9000)"
RUNONCEKEYNAME = "Software\Microsoft\Windows\CurrentVersion\RunOnce"
DiskId1 = "eGalaxTouch Driver Installation Disk(TouchScreen)"
EGALAXTOUCH = "eGalaxTouch"
